# To manually Trigger a port without a pickle switch

*Note: This manually fires a port. It does not trigger a Cue.*

Load show if necessary.

A, Arm All, B

A, Trigger, B

Enter starting port number nn

Press # to fire port and increment port number